# SD/SDIO/MMC 驱动程序

[English]

## 概述

SD/SDIO/MMC 驱动支持 SD 存储器、SDIO 卡和 eMMC 芯片。这是一个协议层驱动 (sdmmc/include/sdmmc_cmd.h)，可以与以下驱动配合使用：

- SDSPI 主机驱动 (esp_driver_sdspi/include/driver/sdspi_host.h)，详情请参阅 SD SPI Host API。

### 协议层与主机层

本文中的 SDMMC 协议层能处理 SD 协议的具体细节，例如卡初始化流程和各种数据传输命令流程。该协议层通过 `sdmmc_host_t` 结构体与主机通信。该结构体包含指向主机各种功能的指针。

主机驱动通过支持以下功能来实现协议驱动：

- 发送命令至从设备

- 接收和发送数据

- 处理总线错误

SD 主机端组件架构

## 应用示例

- storage/sd_card/sdspi 演示了如何通过 SPI 接口操作使用 FatFS 文件系统格式化的 SD 卡。

## 协议层 API

协议层具备 `sdmmc_host_t` 结构体，此结构体描述了 SD/MMC 主机驱动，列出了其功能，并提供指向驱动程序函数的指针。协议层将卡信息储存于 `sdmmc_card_t` 结构体中。向 SD/MMC 主机发送命令时，协议层使用 `sdmmc_command_t` 结构体来描述命令、参数、预期返回值和需传输的数据（如有）。

### 用于 SD 存储卡的 API

- 初始化 SDSPI 主机，请调用主机驱动函数，例如 `sdspi_host_init()` 和 `sdspi_host_init_slot()`。

- 初始化卡，请调用 `sdmmc_card_init()`，并将参数 `host` （主机驱动信息）和参数 `card` （指向 `sdmmc_card_t` 结构体的指针）传递给此函数。函数运行结束后，将会向 `sdmmc_card_t` 结构体填充该卡的信息。

- 读取或写入卡的扇区，请分别调用 `sdmmc_read_sectors()` 和 `sdmmc_write_sectors()`，并将参数 `card` （指向卡信息结构的指针）传递给函数。

- 如果不再使用该卡，请调用主机驱动函数，例如 `sdmmc_host_deinit` 或 `sdspi_host_deinit`，以禁用SDMMC 主机外设或 SDSPI 主机外设，并释放驱动程序分配的资源。

### eMMC 芯片支持

ESP32-C3 没有 SDMMC 主机控制器，只能使用 SPI 协议与卡通信。然而，eMMC 芯片不能通过 SPI 使用。因此，无法在 ESP32-C3 上使用 eMMC 芯片。

### 线程安全

多数应用程序仅需在一个任务中使用协议层。因此，协议层在 `sdmmc_card_t` 结构体或在访问 SDMMC 或 SD SPI 主机驱动程序时不使用任何类型的锁。这种锁通常在较高层级实现，例如文件系统驱动程序。

## API 参考

### Header File

- components/sdmmc/include/sdmmc_cmd.h

- This header file can be included with:

  >     #include "sdmmc_cmd.h"

- This header file is a part of the API provided by the `sdmmc` component. To declare that your component depends on `sdmmc`, add the following to your CMakeLists.txt:

  >     REQUIRES sdmmc

  > or

  >     PRIV_REQUIRES sdmmc

### Functions

esp_err_t sdmmc_card_init(const sdmmc_host_t *host, sdmmc_card_t *out_card)

  Probe and initialize SD/MMC card using given host

  参数:

    - host -- pointer to structure defining host controller

    - out_card -- pointer to structure which will receive information about the card when the function completes

  返回:

    - ESP_OK on success

    - One of the error codes from SDMMC host controller

void sdmmc_card_print_info(FILE *stream, const sdmmc_card_t *card)

  Print information about the card to a stream.

  参数:

    - stream -- stream obtained using fopen or fdopen

    - card -- card information structure initialized using sdmmc_card_init

esp_err_t sdmmc_get_status(sdmmc_card_t *card)

  Get status of SD/MMC card

  参数:

    card -- pointer to card information structure previously initialized using sdmmc_card_init

  返回:

    - ESP_OK on success

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_write_sectors(sdmmc_card_t *card, const void *src, size_t start_sector, size_t sector_count)

  Write given number of sectors to SD/MMC card

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - src -- pointer to data buffer to read data from; data size must be equal to sector_count * card->csd.sector_size

    - start_sector -- sector where to start writing

    - sector_count -- number of sectors to write

  返回:

    - ESP_OK on success or sector_count equal to 0

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_read_sectors(sdmmc_card_t *card, void *dst, size_t start_sector, size_t sector_count)

  Read given number of sectors from the SD/MMC card

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - dst -- pointer to data buffer to write into; buffer size must be at least sector_count * card->csd.sector_size

    - start_sector -- sector where to start reading

    - sector_count -- number of sectors to read

  返回:

    - ESP_OK on success or sector_count equal to 0

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_erase_sectors(sdmmc_card_t *card, size_t start_sector, size_t sector_count, sdmmc_erase_arg_t arg)

  Erase given number of sectors from the SD/MMC card

  备注

  When sdmmc_erase_sectors used with cards in SDSPI mode, it was observed that card requires re-init after erase operation.

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - start_sector -- sector where to start erase

    - sector_count -- number of sectors to erase

    - arg -- erase command (CMD38) argument

  返回:

    - ESP_OK on success or sector_count equal to 0

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_can_discard(sdmmc_card_t *card)

  Check if SD/MMC card supports discard

  参数:

    card -- pointer to card information structure previously initialized using sdmmc_card_init

  返回:

    - ESP_OK if supported by the card/device

    - ESP_FAIL if not supported by the card/device

esp_err_t sdmmc_can_trim(sdmmc_card_t *card)

  Check if SD/MMC card supports trim

  参数:

    card -- pointer to card information structure previously initialized using sdmmc_card_init

  返回:

    - ESP_OK if supported by the card/device

    - ESP_FAIL if not supported by the card/device

esp_err_t sdmmc_mmc_can_sanitize(sdmmc_card_t *card)

  Check if SD/MMC card supports sanitize

  参数:

    card -- pointer to card information structure previously initialized using sdmmc_card_init

  返回:

    - ESP_OK if supported by the card/device

    - ESP_FAIL if not supported by the card/device

esp_err_t sdmmc_mmc_sanitize(sdmmc_card_t *card, uint32_t timeout_ms)

  Sanitize the data that was unmapped by a Discard command

  备注

  Discard command has to precede sanitize operation. To discard, use MMC_DICARD_ARG with sdmmc_erase_sectors argument

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - timeout_ms -- timeout value in milliseconds required to sanitize the selected range of sectors.

  返回:

    - ESP_OK on success

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_full_erase(sdmmc_card_t *card)

  Erase complete SD/MMC card

  参数:

    card -- pointer to card information structure previously initialized using sdmmc_card_init

  返回:

    - ESP_OK on success

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_io_read_byte(sdmmc_card_t *card, uint32_t function, uint32_t reg, uint8_t *out_byte)

  Read one byte from an SDIO card using IO_RW_DIRECT (CMD52)

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - function -- IO function number

    - reg -- byte address within IO function

    - out_byte -- [out] output, receives the value read from the card

  返回:

    - ESP_OK on success

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_io_write_byte(sdmmc_card_t *card, uint32_t function, uint32_t reg, uint8_t in_byte, uint8_t *out_byte)

  Write one byte to an SDIO card using IO_RW_DIRECT (CMD52)

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - function -- IO function number

    - reg -- byte address within IO function

    - in_byte -- value to be written

    - out_byte -- [out] if not NULL, receives new byte value read from the card (read-after-write).

  返回:

    - ESP_OK on success

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_io_read_bytes(sdmmc_card_t *card, uint32_t function, uint32_t addr, void *dst, size_t size)

  Read multiple bytes from an SDIO card using IO_RW_EXTENDED (CMD53)

  This function performs read operation using CMD53 in byte mode. For block mode, see sdmmc_io_read_blocks.

  By default OP Code is set (incrementing address). To send CMD53 without this bit, OR the argument `addr` with `SDMMC_IO_FIXED_ADDR`.

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - function -- IO function number

    - addr -- byte address within IO function where reading starts

    - dst -- buffer which receives the data read from card. Aligned to 4 byte boundary unless `SDMMC_HOST_FLAG_ALLOC_ALIGNED_BUF` flag is set when calling `sdmmc_card_init`. The flag is mandatory when the buffer is behind the cache.

    - size -- number of bytes to read, 1 to 512.

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_SIZE if size exceeds 512 bytes

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_io_write_bytes(sdmmc_card_t *card, uint32_t function, uint32_t addr, const void *src, size_t size)

  Write multiple bytes to an SDIO card using IO_RW_EXTENDED (CMD53)

  This function performs write operation using CMD53 in byte mode. For block mode, see sdmmc_io_write_blocks.

  By default OP Code is set (incrementing address). To send CMD53 without this bit, OR the argument `addr` with `SDMMC_IO_FIXED_ADDR`.

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - function -- IO function number

    - addr -- byte address within IO function where writing starts

    - src -- data to be written. Aligned to 4 byte boundary unless `SDMMC_HOST_FLAG_ALLOC_ALIGNED_BUF` flag is set when calling `sdmmc_card_init`. The flag is mandatory when the buffer is behind the cache.

    - size -- number of bytes to write, 1 to 512.

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_SIZE if size exceeds 512 bytes

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_io_read_blocks(sdmmc_card_t *card, uint32_t function, uint32_t addr, void *dst, size_t size)

  Read blocks of data from an SDIO card using IO_RW_EXTENDED (CMD53)

  This function performs read operation using CMD53 in block mode. For byte mode, see sdmmc_io_read_bytes.

  By default OP Code is set (incrementing address). To send CMD53 without this bit, OR the argument `addr` with `SDMMC_IO_FIXED_ADDR`.

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - function -- IO function number

    - addr -- byte address within IO function where writing starts

    - dst -- buffer which receives the data read from card. Aligned to 4 byte boundary, and also cache line size if the buffer is behind the cache.

    - size -- number of bytes to read, must be divisible by the card block size.

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_SIZE if size is not divisible by 512 bytes

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_io_write_blocks(sdmmc_card_t *card, uint32_t function, uint32_t addr, const void *src, size_t size)

  Write blocks of data to an SDIO card using IO_RW_EXTENDED (CMD53)

  This function performs write operation using CMD53 in block mode. For byte mode, see sdmmc_io_write_bytes.

  By default OP Code is set (incrementing address). To send CMD53 without this bit, OR the argument `addr` with `SDMMC_IO_FIXED_ADDR`.

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - function -- IO function number

    - addr -- byte address within IO function where writing starts

    - src -- data to be written. Aligned to 4 byte boundary, and also cache line size if the buffer is behind the cache.

    - size -- number of bytes to write, must be divisible by the card block size.

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_SIZE if size is not divisible by 512 bytes

    - One of the error codes from SDMMC host controller

esp_err_t sdmmc_io_enable_int(sdmmc_card_t *card)

  Enable SDIO interrupt in the SDMMC host

  参数:

    card -- pointer to card information structure previously initialized using sdmmc_card_init

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if the host controller does not support IO interrupts

esp_err_t sdmmc_io_wait_int(sdmmc_card_t *card, TickType_t timeout_ticks)

  Block until an SDIO interrupt is received

  Slave uses D1 line to signal interrupt condition to the host. This function can be used to wait for the interrupt.

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - timeout_ticks -- time to wait for the interrupt, in RTOS ticks

  返回:

    - ESP_OK if the interrupt is received

    - ESP_ERR_NOT_SUPPORTED if the host controller does not support IO interrupts

    - ESP_ERR_TIMEOUT if the interrupt does not happen in timeout_ticks

esp_err_t sdmmc_io_get_cis_data(sdmmc_card_t *card, uint8_t *out_buffer, size_t buffer_size, size_t *inout_cis_size)

  Get the data of CIS region of an SDIO card.

  You may provide a buffer not sufficient to store all the CIS data. In this case, this function stores as much data into your buffer as possible. Also, this function will try to get and return the size required for you.

  参数:

    - card -- pointer to card information structure previously initialized using sdmmc_card_init

    - out_buffer -- Output buffer of the CIS data

    - buffer_size -- Size of the buffer.

    - inout_cis_size -- Mandatory, pointer to a size, input and output.

      - input: Limitation of maximum searching range, should be 0 or larger than buffer_size. The function searches for CIS_CODE_END until this range. Set to 0 to search infinitely.

      - output: The size required to store all the CIS data, if CIS_CODE_END is found.

  返回:

    - ESP_OK: on success

    - ESP_ERR_INVALID_RESPONSE: if the card does not (correctly) support CIS.

    - ESP_ERR_INVALID_SIZE: CIS_CODE_END found, but buffer_size is less than required size, which is stored in the inout_cis_size then.

    - ESP_ERR_NOT_FOUND: if the CIS_CODE_END not found. Increase input value of inout_cis_size or set it to 0, if you still want to search for the end; output value of inout_cis_size is invalid in this case.

    - and other error code return from sdmmc_io_read_bytes

esp_err_t sdmmc_io_print_cis_info(uint8_t *buffer, size_t buffer_size, FILE *fp)

  Parse and print the CIS information of an SDIO card.

  备注

  Not all the CIS codes and all kinds of tuples are supported. If you see some unresolved code, you can add the parsing of these code in sdmmc_io.c and contribute to the IDF through the Github repository.

               using sdmmc_card_init

  参数:

    - buffer -- Buffer to parse

    - buffer_size -- Size of the buffer.

    - fp -- File pointer to print to, set to NULL to print to stdout.

  返回:

    - ESP_OK: on success

    - ESP_ERR_NOT_SUPPORTED: if the value from the card is not supported to be parsed.

    - ESP_ERR_INVALID_SIZE: if the CIS size fields are not correct.

### Macros

SDMMC_IO_FIXED_ADDR

  Call `sdmmc_io_read_bytes`, `sdmmc_io_write_bytes`, `sdmmc_io_read_blocks` or `sdmmc_io_write_bocks` APIs with address ORed by this flag to send CMD53 with OP Code clear (fixed address)

### Header File

- components/esp_driver_sdmmc/include/driver/sdmmc_types.h

- This header file can be included with:

  >     #include "driver/sdmmc_types.h"

- This header file is a part of the API provided by the `esp_driver_sdmmc` component. To declare that your component depends on `esp_driver_sdmmc`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_driver_sdmmc

  > or

  >     PRIV_REQUIRES esp_driver_sdmmc

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。